Mower straight crop-line fix
- 25m/50m remain TOTAL combined width
- all mower cutting sections share one front and rear WorkArea depth
- start/height stay on the same lateral side per GIANTS WorkArea geometry
- 0.12m neighboring overlap prevents density-map slivers
- mod version remains 1.0.0.1
